**Channel shutter AKP 25**

Shutters for air extraction.

With galvanised protective grille.

Installation instructions

Check to make sure the shutter cannot be accessed when installing in potentially explosive atmospheres.

If it can be touched, pull a finely machined wire cage across the shutter.

Securely earth the wire cage in order to prevent sparks.

Technical data

|  |  |
| --- | --- |
| Article: | AKP 25 |
| Air direction: | Air extraction |
| Loss of pressure: | 10 Pa |
| Installation: | outside |
| Installation site: | Channel |
| Installation position: | vertical / horizontal |
| Material: | Synthetic material, weather and UV resistant |
| Colour: | Light grey |
| Weight: | 1,4 kg |
| Weight including packaging: | 1,805 kg |
| Type of shutter: | Airstream-operated opening/closing |
| Channel dimension: | 500 mm x 300 mm |
| Width: | 585 mm |
| Height: | 385 mm |
| Depth: | 54 mm |
| Width with packaging: | 620 mm |
| Height with packaging: | 400 mm |
| Depth with packaging: | 65 mm |
| Ambient temperature: | 60 °C |
| Packing unit: | 1 piece |
| Range: | D |
| GTIN (EAN): | 4012799510970 |
| Article number: | 0151.0097 |

Manufacturer:

 MAICO

AKP 25 Channel shutter