**Shutter, servomotor VE 50**

Shutters for automatic activation.

Must be combined with additional MS 8 or MS 8 P servomotors (servomotor is not included in the delivery).

Do not use in areas subject to explosions.

Installation instructions

Ensure access to the servomotor.

If required, fit an intermediate piece.

Technical data

|  |  |
| --- | --- |
| Article: | VE 50 |
| Material: | Sheet steel |
| Weight: | 9,765 kg |
| Weight including packaging: | 9,765 kg |
| Type of shutter: | electrical |
| Suitable for nominal size: | 500 mm |
| Width with packaging: | 590 mm |
| Height with packaging: | 520 mm |
| Depth with packaging: | 590 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799932895 |
| Article number: | 0093.0289 |

Manufacturer: MAICO

VE 50 Shutter, servomotor