**Air filter, replacement KF 28-7**

Replacement filter for TFP and TFP -7.

Pocket filter.

Technical data

|  |  |
| --- | --- |
| Article: | KF 28-7 |
| Installation position: | vertical / horizontal |
| Weight: | 1,9 kg |
| Weight including packaging: | 2,47 kg |
| Filter class: | ISO ePM1 80 % (F7) |
| Channel dimension: | 600 mm x 300 mm |
| Width: | 610 mm |
| Height: | 295 mm |
| Depth: | 320 mm |
| Width with packaging: | 611 mm |
| Height with packaging: | 300 mm |
| Depth with packaging: | 321 mm |
| Ambient temperature: | 70 °C |
| Packing unit: | 2 pieces |
| Range: | D |
| GTIN (EAN): | 4012799938651 |
| Article number: | 0093.0865 |

Manufacturer: MAICO

KF 28-7 Air filter, replacement