**Fan insert VE ER-APB 60**

Fan insert as spare part for surface-mounted fan, fire protection ER-APB 60.

Standard model.

Technical data

|  |  |
| --- | --- |
| Article: | VE ER-APB 60 |
| Model: | Standard model |
| Air flow volume: | 61 m³/h |
| Rotating speed: | 1.250 1/min |
| Speed controllable: | - |
| Type of voltage: | Alternating current |
| Rated voltage: | 230 V |
| Frequency: | 50 Hz |
| Nominal output: | 21 W |
| Imax: | 0,17 A |
| Degree of protection: | IP X5 |
| Colour: | white |
| Weight: | 1 kg |
| Weight including packaging: | 1,33 kg |
| Width: | 215 mm |
| Height: | 110 mm |
| Depth: | 215 mm |
| Width with packaging: | 270 mm |
| Height with packaging: | 155 mm |
| Depth with packaging: | 280 mm |
| Range: | B |
| GTIN (EAN): | 4012799100966 |
| Article number: | E084.0156.0000 |

Manufacturer: MAICO

VE ER-APB 60 Fan insert