**Air filter, replacement KF 28**

Replacement filter for TFP and TFP -7.

Pocket filter.

Technical data

|  |  |
| --- | --- |
| Article: | KF 28 |
| Installation position: | vertical / horizontal |
| Weight: | 1,57 kg |
| Weight including packaging: | 2,96 kg |
| Filter class: | ISO Coarse 85 % (G4) |
| Channel dimension: | 600 mm x 300 mm |
| Width: | 610 mm |
| Height: | 295 mm |
| Depth: | 270 mm |
| Width with packaging: | 625 mm |
| Height with packaging: | 335 mm |
| Depth with packaging: | 625 mm |
| Ambient temperature: | 70 °C |
| Packing unit: | 2 pieces |
| Range: | D |
| GTIN (EAN): | 4012799936831 |
| Article number: | 0093.0683 |

Manufacturer: MAICO

KF 28 Air filter, replacement