**Air filter, replacement KF 31**

Replacement filter for TFP and TFP -7.

Pocket filter.

Technical data

|  |  |
| --- | --- |
| Article: | KF 31 |
| Installation position: | vertical / horizontal |
| Weight: | 1,86 kg |
| Weight including packaging: | 3,37 kg |
| Filter class: | ISO Coarse 85 % (G4) |
| Channel dimension: | 600 mm x 350 mm |
| Width: | 610 mm |
| Height: | 345 mm |
| Depth: | 350 mm |
| Width with packaging: | 620 mm |
| Height with packaging: | 430 mm |
| Depth with packaging: | 620 mm |
| Ambient temperature: | 70 °C |
| Packing unit: | 2 pieces |
| Range: | D |
| GTIN (EAN): | 4012799936848 |
| Article number: | 0093.0684 |

Manufacturer: MAICO

KF 31 Air filter, replacement