**Recessed-mounted housing ER GH**

Special features

Exhaust socket can be converted, without tools, from “side” to “rear”.

Lateral mounting grooves for installation with mounting brackets or in front wall installations.

Airstream-operated plastic backflow preventer with simultaneous function as a cold smoke barrier.

For applications in accordance with DIN 18017-3.

Single-room air extraction

Installation in bathrooms, WCs and open-plan kitchens.

Installation inside and outside the wall and ceiling shafts is possible.

Reduced overall depth of the flush-mounted housing and the cover.

6 laterally attached mounting grooves allow for easy installation.

Circumferential frame allows for additional fixing options.

Flexible cable entry allows electrical connection from the side or rear.

Simple electrical wiring on practical pin connector terminal.

With plaster protective cover to close the housing during the shell construction phase.

Plastic exhaust socket with airstream-operated plastic backflow preventer can be converted, without tools, for air outlet direction to the side (top, left, right) and rear.

DN 75/80 connection diameter.

Knockout points for second room connection or WC connection socket, as a standard feature, in the ER GH housing.

Certificates of approval on request or on our website – www.maico-ventilatoren.com.

Plastic parts, normally inflammable, according to DIN 4102-1 class B 2 (according to EN 13501-1).

Optional accessories

ER-AS extraction socket for the toilet seat air extraction

ER-ZR second room connection

ER-MS installation kit

ER-UPM mounting support

Technical data

|  |  |
| --- | --- |
| Article: | ER GH |
| Model: | Plastic exhaust socket, convertible at side/rear, with airstream-operated plastic backflow preventer, without fire protection housing, second room connection possible on right/left/at bottom |
| Air direction: | Air extraction |
| Installation site: | Wall / Ceiling |
| Type of installation: | Recessed-mounted |
| Housing material: | Synthetic material |
| Colour: | Black |
| Weight: | 0,59 kg |
| Weight including packaging: | 0,89 kg |
| Fire protection: | No |
| Air outlet direction: | at side / at rear |
| Connection diameter: | 75 mm / 80 mm |
| Width: | 250 mm |
| Height: | 250 mm |
| Depth: | 110 mm |
| Width with packaging: | 350 mm |
| Height with packaging: | 290 mm |
| Depth with packaging: | 130 mm |
| Approval number: | Z-51.1-478 |
| Packing unit: | 1 piece |
| Range: | B |
| GTIN (EAN): | 4012799843504 |
| Article number: | 0084.0350 |

Manufacturer: MAICO

ER GH Recessed-mounted housing