**External cover PPB 30 AK**

Plastic external cover.

Colour: traffic white, similar to RAL 9016.

The grille lamellae are flow-optimised to minimise air disturbances and the exhaust air is kept away from the exterior wall. This greatly minimises discolouration and dirt deposits on the external façade.

An external cover is needed as an accessory for the PPB 30 K and PPB 30 O final installation kits.

Technical data

|  |  |
| --- | --- |
| Article: | PPB 30 AK |
| Installation site: | Outside wall |
| Installation position: | horizontal |
| Material: | Synthetic material |
| Housing material: | Synthetic material |
| Colour: | Traffic white, similar to RAL 9016 |
| Weight: | 0,85 kg |
| Weight including packaging: | 1,06 kg |
| Width: | 275 mm |
| Height: | 275 mm |
| Depth: | 65 mm |
| Width with packaging: | 295 mm |
| Height with packaging: | 320 mm |
| Depth with packaging: | 87 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799991755 |
| Article number: | 0093.1498 |

Manufacturer: MAICO

PPB 30 AK External cover