**Flexible coupling ELI 90 Ex**

Dampens vibrations along the channel system.

Strong and flexible fabric seal.

Protected against weathering by epoxy coating.

Suitable for operating temperatures from -30 °C to +80 °C.

Technical data

|  |  |
| --- | --- |
| Article: | ELI 90 Ex |
| Material: | Sheet steel, epoxy coated |
| Colour: | grey |
| Weight: | 23 kg |
| Weight including packaging: | 23 kg |
| Width: | 1.030 mm |
| Height: | 908 mm |
| Depth: | 203 mm |
| Width with packaging: | 1.030 mm |
| Height with packaging: | 908 mm |
| Depth with packaging: | 203 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799735816 |
| Article number: | 0073.0581 |

Manufacturer: MAICO

ELI 90 Ex Flexible coupling