**Internal grille LGA 62/22**

Internal grille with front frame.

With vertical, rotatable air operated lamella with fitted bearings, located on the front side.

Air flow control by means of adjustable slot slides.

Accessories needed: EK installation box.

Technical data

|  |  |
| --- | --- |
| Article: | LGA 62/22 |
| Air direction: | Air extraction |
| Practical air throughput at 75% opening of the slot slide: | 300 m³/h - 1000 m³/h |
| Installation: | Inside |
| Installation site: | Wall / Channel |
| Material: | Sheet steel, stove-enamelled |
| Colour: | light grey |
| Weight: | 3,71 kg |
| Weight including packaging: | 4,11 kg |
| Width: | 650 mm |
| Height: | 260 mm |
| Depth: | 61 mm |
| Width with packaging: | 680 mm |
| Height with packaging: | 275 mm |
| Depth with packaging: | 95 mm |
| Packing unit: | 1 piece |
| Range: | D |
| GTIN (EAN): | 4012799512622 |
| Article number: | 0151.0262 |

Manufacturer: MAICO

LGA 62/22 Internal grille