**Dongle ER DIP EC**

Parametrizable dongle for individual adaptation of the ER EC function.

Parameter settings:

V1 volumetric flow in 5 m³/h steps

V2 volumetric flow in 5 m³/h steps

Te start delay in 10 sec. steps

Ta overrun time in 5 min steps

Ti interval time in 1 h steps

BI operating time in 5 min steps

Fulfils the system’s IP protection: IP X5

Technical data

|  |  |
| --- | --- |
| Article: | ER DIP EC |
| Installation site: | ER EC fan insert |
| Type of installation: | Surface or recess mounting |
| Material: | Plastic / rubber |
| Colour: | Black |
| Weight: | 0,01 kg |
| Width: | 25 mm |
| Height: | 16 mm |
| Depth: | 130 mm |
| Packing unit: | depending on the order, from 15 items |
| Range: | B |
| GTIN (EAN): | 4012799992592 |
| Article number: | 0157.1648 |

Manufacturer: MAICO

ER DIP EC Dongle