**Shutter, manual RS 60**

Shutters for air extraction and ventilation.

Lamella can be operated manually or with an additional MS 2 servomotor.

From nominal size 35 with centre bridge for increasing the stability of the shutters.

With pulley, 2.5 m pull cord and pull-cord clip.

With galvanised protective grille.

Recommended accessories: ZVR connection frames for mounting the AS and RS shutters to the fan rather than the wall.

Technical data

|  |  |
| --- | --- |
| Article: | RS 60 |
| Air direction: | Ventilation and air extraction |
| Installation: | outside |
| Installation site: | Wall |
| Installation position: | vertical |
| Material: | Synthetic material, weather and UV resistant |
| Colour: | Traffic white, similar to RAL 9016 |
| Lamella colour: | Silver grey |
| Weight: | 3,68 kg |
| Weight including packaging: | 4,22 kg |
| Type of shutter: | electrical / manual |
| Nominal size: | 600 mm |
| Width: | 684 mm |
| Height: | 684 mm |
| Depth: | 42 mm |
| Width with packaging: | 750 mm |
| Height with packaging: | 700 mm |
| Depth with packaging: | 50 mm |
| Ambient temperature: | 60 °C |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799513452 |
| Article number: | 0151.0345 |

Manufacturer: MAICO

RS 60 Shutter, manual