**Safety isolating transformer TRE 50**

Safety isolating transformer

for connecting an ECA 120 24 V

or in conjunction with the SKD CO2sensor

or in conjunction with the FFT 30 K humidity and temperature sensor.

Insulation class T 40 E.

Designed according to VDE 0551.

With exchangeable glass tube fuse for conditional short circuit strength.

Technical data

|  |  |
| --- | --- |
| Article: | TRE 50 |
| Type of voltage: | Alternating current |
| Rated voltage: | 230 V |
| Frequency: | 50 Hz/60 Hz |
| Power consumption (without speed control): | 50 W |
| Imax: | 1 A |
| Maximum load (ohmic load): | 2,1 A |
| Degree of protection: | IP 20 |
| Secondary voltage: | 24 V |
| Type of installation: | Control cabinet |
| Housing material: | Synthetic material |
| Weight: | 1 kg |
| Weight including packaging: | 1,1 kg |
| Width with packaging: | 125 mm |
| Height with packaging: | 85 mm |
| Depth with packaging: | 80 mm |
| Packing unit: | 1 piece |
| Range: | A |
| GTIN (EAN): | 4012799573852 |
| Article number: | 0157.0385 |

Manufacturer: MAICO

TRE 50 Safety isolating transformer