**Sound-absorbing element set ER-SE EC**

Serves as a sound absorber and reduces the noise emissions.

For retrofitting ER EC fan inserts. With cover frame

Simple to install.

Construction material class B1.

Technical data

|  |  |
| --- | --- |
| Article: | ER-SE EC |
| Installation site: | Housing over the fan insert |
| Material: | plastic, malamine resin foam |
| Colour: | traffic white, similar to RAL 9016, grey |
| Weight: | 0,2 kg |
| Weight including packaging: | 0,49 kg |
| Width: | 305 mm |
| Height: | 305 mm |
| Depth: | 60 mm |
| Width with packaging: | 375 mm |
| Height with packaging: | 375 mm |
| Depth with packaging: | 110 mm |
| Total insertion loss: | 1,5 dB |
| Insertion loss note: | max. 5.5 dB |
| Packing unit: | 1 piece |
| Range: | B |
| GTIN (EAN): | 4012799992356 |
| Article number: | 0093.1565 |

Manufacturer: MAICO

ER-SE EC Sound-absorbing element set