**Bracket MF-WLF125/90**

MF-WLF100/90: Direct 90° adaptor from round cross-section (supply air or exhaust air valve) NW 100 to MF-F90 flexible steel duct.

MF-WLF125/90: Direct 90° adaptor from round cross-section (supply air or exhaust air valve) NW 125 to MF-F90 flexible steel duct.

MF-WLF100/63/63: Direct 90° adaptor with very low height (70 mm) from round cross-section (supply air or exhaust air valve) NW 100 to two MF-F63 flexible steel ducts.

Valve connection sockets with collar size.

The flexible steel duct connection sockets each have two push-in mounting brackets which allow the flexible steel ducts to be fixed quickly and cheaply.

Technical data

|  |  |
| --- | --- |
| Article: | MF-WLF125/90 |
| Air direction: | Ventilation and air extraction |
| Installation site: | Ceiling / Wall / Floor |
| Material: | Sheet steel, galvanised |
| Weight: | 1,1 kg |
| Weight including packaging: | 1,12 kg |
| Nominal size: | 125 mm / 90 mm |
| Width: | 240 mm |
| Height: | 410 mm |
| Depth: | 300 mm |
| Width with packaging: | 240 mm |
| Height with packaging: | 410 mm |
| Depth with packaging: | 300 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799185291 |
| Article number: | 0018.0529 |

Manufacturer: MAICO

MF-WLF125/90 Bracket