**Air filter, replacement ALDF 12 G2**

ALDF 12 G2: Replacement filter for ALD 12 S and ALD 12 SVA outside air opening.

ALDF 12 G3: Replacement filter for ALD 12 S and ALD 12 SVA outside air opening.

Technical data

|  |  |
| --- | --- |
| Article: | ALDF 12 G2 |
| Installation position: | vertical / horizontal |
| Weight: | 0,01 kg |
| Weight including packaging: | 0,05 kg |
| Type of filter: | Dust filter |
| Filter class: | ISO Coarse 30 % (G2) |
| Width: | 140 mm |
| Height: | 140 mm |
| Depth: | 12 mm |
| Width with packaging: | 141 mm |
| Height with packaging: | 141 mm |
| Depth with packaging: | 60 mm |
| Ambient temperature: | 60 °C |
| Packing unit: | 5 pieces |
| Suitable for products: | ALD 12 S / ALD 12 SVA |
| Range: | B |
| GTIN (EAN): | 4012799931522 |
| Article number: | 0093.0152 |

Manufacturer: MAICO

ALDF 12 G2 Air filter, replacement