**Air filter TFP 35-7**

Air filter for ventilation systems.

Flanges on both sides for installation in square ventilation channels.

Inspection lid can be removed for easy filter exchange.

Accessories: KF.. replacement air filter and DW 1000 differential pressure controller.

Installation instructions

Mount the air filter on the fan's suction side.

Monitor filter resistance using DW 1000 differential pressure controller.

Provide sufficient space on the side for opening the inspection lid during a filter change.

Technical data

|  |  |
| --- | --- |
| Article: | TFP 35-7 |
| Installation site: | Channel |
| Installation position: | vertical / horizontal |
| Housing material: | Sheet steel, galvanised |
| Weight: | 14,4 kg |
| Weight including packaging: | 14,41 kg |
| Type of filter: | Dust and pollen filter |
| Filter class: | ISO ePM1 80 % (F7) |
| Channel dimension: | 700 mm x 400 mm |
| Width: | 740 mm |
| Height: | 440 mm |
| Depth: | 600 mm |
| Width with packaging: | 740 mm |
| Height with packaging: | 440 mm |
| Depth with packaging: | 600 mm |
| Airstream temperature at IMax: | 70 °C |
| Packing unit: | 1 piece |
| Range: | D |
| GTIN (EAN): | 4012799490715 |
| Article number: | 0149.0071 |

Manufacturer: MAICO

TFP 35-7 Air filter