**Air filter, replacement PP 45 G2**

Replacement air filter for PushPull 45 single-room ventilation unit.

The ISO Coarse 30 % (G2) filters are installed on the inside and the ISO Coarse 45 % (G3) filters on the outside.

Technical data

|  |  |
| --- | --- |
| Article: | PP 45 G2 |
| Material: | Synthetic |
| Colour: | white |
| Weight: | 0,01 kg |
| Weight including packaging: | 0,01 kg |
| Filter class: | ISO Coarse 30 % (G2) |
| Width: | 140 mm |
| Height: | 140 mm |
| Depth: | 10 mm |
| Width with packaging: | 200 mm |
| Height with packaging: | 180 mm |
| Depth with packaging: | 22 mm |
| Packing unit: | 2 pieces |
| Range: | K |
| GTIN (EAN): | 4012799932734 |
| Article number: | 0093.0273 |

Manufacturer: MAICO

PP 45 G2 Air filter, replacement