**5-step transformer, control cabinet TRE 1,6 S-2**

5-step transformers for setting speed.

To control AC fans.

With foot bracket and connection terminals.

With profile rail for integral transformers < 3 kg.

Accessories: ESS 20 5-step switch

Technical data

|  |  |
| --- | --- |
| Article: | TRE 1,6 S-2 |
| Type of voltage: | Alternating current |
| Rated voltage: | 230 V |
| Frequency: | 50 Hz/60 Hz |
| Nominal output: | 288 W |
| Maximum load: | 1,6 A |
| Degree of protection: | IP 00 |
| Secondary voltage: | 85 V / 115 V / 150 V / 180 V / 230 V |
| Type of installation: | Control cabinet |
| Weight: | 1,96 kg |
| Weight including packaging: | 2,84 kg |
| Width: | 84 mm |
| Height: | 75 mm |
| Depth: | 95 mm |
| Width with packaging: | 240 mm |
| Height with packaging: | 230 mm |
| Depth with packaging: | 190 mm |
| Ambient temperature: | 0 °C up to 40 °C |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799571629 |
| Article number: | 0157.0162 |

Manufacturer: MAICO

TRE 1,6 S-2 5-step transformer, control cabinet