**Stainless steel cowl LH-V2A 15**

Cowl for ventilation and air extraction.

For connecting to exhaust air ducts, extraction hoods, tumble dryers, etc.

With connection socket and spring clamp for simple installation.

With bird protection grille.

No lip seal on socket and no condensation run-off catcher.

If the cowl is used as outgoing air device, the customer must take action to ensure that any condensation produced does not drain onto the building facade.

Technical data

|  |  |
| --- | --- |
| Article: | LH-V2A 15 |
| Air direction: | Ventilation and air extraction |
| Installation: | outside |
| Installation site: | Outside wall |
| Material: | Stainless steel |
| Colour: | Stainless steel, brushed |
| Weight: | 0,4 kg |
| Weight including packaging: | 0,4 kg |
| Suitable for nominal size: | 150 mm |
| Open cross section: | 146 cm² |
| Width: | 212 mm |
| Height: | 212 mm |
| Depth: | 52 mm |
| Width with packaging: | 215 mm |
| Height with packaging: | 215 mm |
| Depth with packaging: | 170 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799513797 |
| Article number: | 0151.0379 |

Manufacturer: MAICO

LH-V2A 15 Stainless steel cowl