**Fan insert with cover VEA ER 17/60-1 VZ**

Fan insert, cover with fixed internal grille and filter as spare part for ER 17/60-1 VZ fan insert.

Model with time delay switch.

Technical data

|  |  |
| --- | --- |
| Article: | VEA ER 17/60-1 VZ |
| Model: | Time delay switch |
| Air flow volume: | 61 m³/h |
| Rotating speed: | 2.500 1/min |
| Speed controllable: | - |
| Type of voltage: | Alternating current |
| Rated voltage: | 230 V |
| Frequency: | 50 Hz |
| Nominal output: | 46 W |
| Imax: | 0,3 A |
| Colour: | white |
| Weight: | 1,62 kg |
| Weight including packaging: | 1,93 kg |
| Width: | 245 mm |
| Height: | 145 mm |
| Depth: | 245 mm |
| Width with packaging: | 270 mm |
| Height with packaging: | 155 mm |
| Depth with packaging: | 280 mm |
| Range: | B |
| GTIN (EAN): | 4012799991465 |
| Article number: | E080.0781.0000 |

Manufacturer: MAICO

VEA ER 17/60-1 VZ Fan insert with cover