**Air filter, replacement RF 25**

Replacement filter for TFE... air filter.

Technical data

|  |  |
| --- | --- |
| Article: | RF 25 |
| Installation position: | vertical / horizontal |
| Weight: | 0,29 kg |
| Weight including packaging: | 0,31 kg |
| Filter class: | ISO Coarse 70 % (G4) |
| Suitable for nominal size: | 250 mm |
| Width: | 294 mm |
| Height: | 215 mm |
| Depth: | 6 mm |
| Width: | 295 mm |
| Height: | 295 mm |
| Width with packaging: | 320 mm |
| Height with packaging: | 295 mm |
| Depth with packaging: | 35 mm |
| Ambient temperature: | 100 °C |
| Packing unit: | 2 pieces |
| Range: | C |
| GTIN (EAN): | 4012799936947 |
| Article number: | 0093.0694 |

Manufacturer: MAICO

RF 25 Air filter, replacement