**Air filter, replacement KF 35-7**

Replacement filter for TFP and TFP -7.

Pocket filter.

Technical data

|  |  |
| --- | --- |
| Article: | KF 35-7 |
| Installation position: | vertical / horizontal |
| Weight: | 2,62 kg |
| Weight including packaging: | 4,2 kg |
| Filter class: | ISO ePM1 80 % (F7) |
| Channel dimension: | 700 mm x 400 mm |
| Width: | 700 mm |
| Height: | 400 mm |
| Depth: | 370 mm |
| Width with packaging: | 625 mm |
| Height with packaging: | 625 mm |
| Depth with packaging: | 420 mm |
| Ambient temperature: | 70 °C |
| Packing unit: | 2 pieces |
| Range: | D |
| GTIN (EAN): | 4012799938675 |
| Article number: | 0093.0867 |

Manufacturer: MAICO

KF 35-7 Air filter, replacement