**External cover PPB 30 AW**

External cover made of aluminium.

Colour: white powder coated, similar to RAL 9010.

The integrated air-redirection keeps the exhaust air away from the exterior wall. This greatly minimises discolouration and dirt deposits on the external façade.

Is recommended when the units are used in areas exposed to the wind.

An external cover is needed as an accessory for the PPB 30 K and PPB 30 O final installation kits.

Technical data

|  |  |
| --- | --- |
| Article: | PPB 30 AW |
| Installation site: | Outside wall |
| Installation position: | horizontal |
| Housing material: | Aluminium |
| Colour: | White powder-coated, similar to RAL 9010 |
| Weight: | 0,76 kg |
| Weight including packaging: | 0,96 kg |
| Width: | 253 mm |
| Height: | 258 mm |
| Depth: | 67 mm |
| Width with packaging: | 295 mm |
| Height with packaging: | 320 mm |
| Depth with packaging: | 86 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799991779 |
| Article number: | 0093.1500 |

Manufacturer: MAICO

PPB 30 AW External cover