**Shutter ARP 71**

Shutters for air extraction.

With individually moving lamella, fitted using reinforced bushing.

With galvanised protective grille on the inflow side.

Two-part ARP 71.

Three-part ARP 80 and ARP 100.

Technical data

|  |  |
| --- | --- |
| Article: | ARP 71 |
| Air direction: | Air extraction |
| Installation: | outside |
| Installation site: | Wall |
| Installation position: | vertical / horizontal |
| Material: | Synthetic material, weather and UV resistant |
| Colour: | Silver grey |
| Weight: | 4,6 kg |
| Weight including packaging: | 5,6 kg |
| Type of shutter: | Airstream-operated opening/closing |
| Suitable for nominal size: | 710 mm |
| Width: | 818 mm |
| Height: | 890 mm |
| Depth: | 40 mm |
| Width with packaging: | 900 mm |
| Height with packaging: | 900 mm |
| Depth with packaging: | 55 mm |
| Ambient temperature: | 60 °C |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799510826 |
| Article number: | 0151.0082 |

Manufacturer:
MAICO

ARP 71 Shutter