**Exhaust air silencer SDA 31**

Sound absorber for pressure side sound insulation of ERD and DRD roof fans.

With silencing elements made of water repellent and non-flammable material.

Easy installation - retrofit installation is also possible.

Technical data

|  |  |
| --- | --- |
| Article: | SDA 31 |
| Loss of pressure: | 5 Pa |
| Installation site: | Roof |
| Housing material: | Sheet steel, galvanised |
| Weight: | 38,5 kg |
| Weight including packaging: | 43,5 kg |
| Suitable for nominal size: | 315 mm |
| Width: | 720 mm |
| Height: | 1.047 mm |
| Depth: | 720 mm |
| Width with packaging: | 750 mm |
| Height with packaging: | 580 mm |
| Depth with packaging: | 750 mm |
| Ambient temperature: | 100 °C |
| Insertion loss at 125 Hz: | 8 dB |
| Insertion loss at 250 Hz: | 2 dB |
| Insertion loss at 500 Hz: | 12 dB |
| Insertion loss at 1 kHz: | 15 dB |
| Insertion loss at 2 kHz: | 13 dB |
| Insertion loss at 4 kHz: | 17 dB |
| Insertion loss at 8 kHz: | 16 dB |
| Total insertion loss: | 9 dB |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799923886 |
| Article number: | 0092.0388 |

Manufacturer: MAICO

SDA 31 Exhaust air silencer