**External grille LAP 56**

External grille for air extraction and ventilation.

With fixed rain-repellent weather protection lamella.

With frame for mounting in masonry walls.

Protective grille in accordance with DIN EN ISO 13857.

Technical data

|  |  |
| --- | --- |
| Article: | LAP 56 |
| Air direction: | Ventilation and air extraction |
| Installation: | outside |
| Installation site: | Wall / Channel |
| Material: | Aluminium |
| Colour: | Anodised aluminium |
| Weight: | 11,4 kg |
| Weight including packaging: | 12,18 kg |
| Channel dimension: | 1.000 mm x 500 mm |
| Width: | 1.029 mm |
| Height: | 575 mm |
| Depth: | 73 mm |
| Width with packaging: | 1.090 mm |
| Height with packaging: | 590 mm |
| Depth with packaging: | 110 mm |
| Packing unit: | 1 piece |
| Range: | D |
| GTIN (EAN): | 4012799513131 |
| Article number: | 0151.0313 |

Manufacturer: MAICO

LAP 56 External grille