**Bypass for heat exchanger WS-BPR 320/470**

Automatic 100% bypass with position feedback for WR 310 R/WR 410 R, WS 320 R and WS 470 R centralised ventilation units.

Technical data

|  |  |
| --- | --- |
| Article: | WS-BPR 320/470 |
| Material: | EPP |
| Weight: | 1,32 kg |
| Weight including packaging: | 2,02 kg |
| Width: | 193 mm |
| Height: | 95 mm |
| Depth: | 505 mm |
| Width with packaging: | 350 mm |
| Height with packaging: | 170 mm |
| Depth with packaging: | 515 mm |
| Packing unit: | 1 piece |
| Suitable for products: | WS 320 R..., WS 470 R..., WR 310 R, WR 410 R |
| Range: | K |
| GTIN (EAN): | 4012799992417 |
| Article number: | 0093.1577 |

Manufacturer: MAICO

WS-BPR 320/470 Bypass for heat exchanger