**Storm protection ALDS 10**

Storm protection for air flow regulation with strong or gusty winds.

Accessories for ALD 10 outside air openings.

Mounted by sliding into wall sleeve.

Installation instructions

In the case of detached buildings it is recommended that installation be made on the weather side and from the 3rd floor upwards.

Technical data

|  |  |
| --- | --- |
| Article: | ALDS 10 |
| Housing material: | Polystyrene |
| Membrane material: | Special silicone |
| Weight: | 0,05 kg |
| Weight including packaging: | 0,06 kg |
| Suitable for nominal size: | 100 mm |
| Width: | 120 mm |
| Height: | 120 mm |
| Depth: | 90 mm |
| Width with packaging: | 200 mm |
| Height with packaging: | 80 mm |
| Depth with packaging: | 200 mm |
| Packing unit: | 1 piece |
| Range: | B |
| GTIN (EAN): | 4012799520566 |
| Article number: | 0152.0056 |

Manufacturer: MAICO

ALDS 10 Storm protection