**Fire protection ceiling barrier TS 18 DN 160**

Fire protection ceiling barrier for ER exhaust air systems.

With continuous open cross-section and smooth inner surfaces.

General official approval, approval number Z-41.3-556.

Certificate of approval at www.maico-fans.com.

Fire resistance class K90-18017.

Maintenance-free.

Technical data

|  |  |
| --- | --- |
| Article: | TS 18 DN 160 |
| Air direction: | Ventilation and air extraction |
| Installation site: | Ceiling |
| Type of installation: | Recessed-mounted |
| Material: | Sheet steel |
| Weight: | 2,08 kg |
| Weight including packaging: | 2,1 kg |
| Fire protection: | yes |
| Suitable for nominal size: | 160 mm |
| Width: | 295 mm |
| Height: | 180 mm |
| Depth: | 195 mm |
| Width with packaging: | 296 mm |
| Height with packaging: | 181 mm |
| Depth with packaging: | 196 mm |
| Approval number: | Z-41.3-556 |
| Packing unit: | 1 piece |
| Range: | B |
| GTIN (EAN): | 4012799513230 |
| Article number: | 0151.0323 |

Manufacturer: MAICO

TS 18 DN 160 Fire protection ceiling barrier