**Air filter, replacement RF 16-4**

Replacement filter for TFE...-4 air filter.

Technical data

|  |  |
| --- | --- |
| Article: | RF 16-4 |
| Installation position: | vertical / horizontal |
| Weight: | 0,203 kg |
| Weight including packaging: | 0,223 kg |
| Filter class: | G4 |
| Suitable for nominal size: | 160 mm |
| Width: | 280 mm |
| Height: | 175 mm |
| Width with packaging: | 410 mm |
| Height with packaging: | 40 mm |
| Depth with packaging: | 280 mm |
| Ambient temperature: | 100 °C |
| Packing unit: | 2 pieces |
| Range: | C |
| GTIN (EAN): | 4012799930716 |
| Article number: | 0093.0071 |

Manufacturer: MAICO

RF 16-4 Air filter, replacement