**Cover ER-A**

ER-A – standard model

Standard cover for ER EC with filter change indicator (time strip).

Base load: 30 m³/h / full load 60 m³/h.

Full load level on/off via light switch or separate switch.

Switching to full load level (60 m³/h) with start delay of approx. 60 sec.

Full load overrun time approx. 15 min.

Special features

Flow-optimised, attractive design

Filter can be changed without tools.

With filter change indicator.

Features

The unit can be run in continuous operation at the base load level.

IP X5 degree of protection for safety in the bathroom.

Colour: traffic white, similar to RAL 9016.

For single-room air extraction using a single fan.

ISO Coarse 30 % filter (G2), filter change without tools.

It is possible to rotate the cover by ± 5°, to compensate for housings which have been fitted at an angle.

Not speed controllable.

Switching option: The base load can be switched on or off by an additional switch (see the wiring diagrams online).

\*Factory settings

Technical data

|  |  |
| --- | --- |
| Article: | ER-A |
| Model: | Standard |
| Air flow volume: | 30 m³/h / 60 m³/h (Level 1/level 2) |
| Air direction: | Air extraction |
| Degree of protection: | IP X5 |
| Installation site: | Wall / Ceiling |
| System type: | Decentralised |
| Housing material: | Synthetic material |
| Colour: | Traffic white, similar to RAL 9016 |
| Weight: | 0,47 kg |
| Weight including packaging: | 0,62 kg |
| Filter class: | ISO Coarse 30 % (G2) |
| Width: | 281 mm |
| Height: | 281 mm |
| Depth: | 33 mm |
| Width with packaging: | 310 mm |
| Height with packaging: | 300 mm |
| Depth with packaging: | 40 mm |
| Airstream temperature at IMax: | 40 °C |
| Start delay: | 60 s |
| Sound pressure level: | 15 dB(A) / 35 dB(A) combined with ER GH; 31 dB(A) / 41 dB(A) combined with ER GH AP/APB/ Specification according to DIN 18017-3 with an equivalent absorption area AL = 10 m² |
| Approval number: | Z-51.1-478 |
| Packing unit: | 1 piece |
| Range: | B |
| GTIN (EAN): | 4012799843610 |
| Article number: | 0084.0361 |

Manufacturer: MAICO

ER-A Cover