**Room air control ZEG EC-FB**

Additional wireless remote control with humidity sensor activation for ZEG EC exhaust air unit.

The remote control can be installed in damp rooms - but not in the shower cubicle itself.

The remote control must not be sprayed (relative humidity of less than 90 %).

Technical data

|  |  |
| --- | --- |
| Article: | ZEG EC-FB |
| Type of voltage: | Alternating current |
| Battery: | Type 3 V CR 2025 |
| Mains cable: | not required |
| Type of installation: | Surface-mounted |
| Material: | Synthetic material |
| Synthetic material definition: | PVC-free polystyrene |
| Colour: | White, similar to RAL 9010 |
| Weight: | 0,075 kg |
| Weight including packaging: | 0,1 kg |
| Width: | 82 mm |
| Height: | 82 mm |
| Depth: | 18 mm |
| Width with packaging: | 88 mm |
| Height with packaging: | 88 mm |
| Depth with packaging: | 25 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799574118 |
| Article number: | 0157.0411 |

Manufacturer: MAICO

ZEG EC-FB Room air control