**Temperature control system, power module ATL 2,5**

Power module for ATS electronic 2 point thermostat for controlling the 3-phase AC fans.

5-step transformer, with optional automatic setting via temperature controller or manual setting.

Technical data

|  |  |
| --- | --- |
| Article: | ATL 2,5 |
| Rated voltage: | 400 V |
| Frequency: | 50 Hz/60 Hz |
| Maximum load: | 2,5 A |
| Degree of protection: | IP 54 |
| Secondary voltage: | 110 V / 150 V / 190 V / 250 V / 400 V |
| Type of installation: | Surface-mounted |
| Housing material: | Synthetic material |
| Colour: | Light grey |
| Weight: | 17,5 kg |
| Weight including packaging: | 18,2 kg |
| Width: | 300 mm |
| Height: | 400 mm |
| Depth: | 160 mm |
| Width with packaging: | 490 mm |
| Height with packaging: | 195 mm |
| Depth with packaging: | 400 mm |
| Ambient temperature: | 40 °C |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799577577 |
| Article number: | 0157.0757 |

Manufacturer: MAICO

ATL 2,5 Temperature control system, power module