**Fan insert with cover VEA ER 17/60-2**

Fan insert with cover and filter as spare part for ER 17/60-2 fan insert.

Standard model.

Technical data

|  |  |
| --- | --- |
| Article: | VEA ER 17/60-2 |
| Model: | Standard model |
| Air flow volume: | 61 m³/h |
| Rotating speed: | 2.500 1/min |
| Speed controllable: |  ✔  |
| Type of voltage: | Alternating current |
| Rated voltage: | 230 V |
| Frequency: | 50 Hz |
| Nominal output: | 46 W |
| Imax: | 0,3 A |
| Colour: | white |
| Weight: | 1,98 kg |
| Weight including packaging: | 2,21 kg |
| Width: | 250 mm |
| Height: | 170 mm |
| Depth: | 250 mm |
| Width with packaging: | 260 mm |
| Height with packaging: | 180 mm |
| Depth with packaging: | 260 mm |
| Range: | B |
| GTIN (EAN): | 4012799991113 |
| Article number: | E080.0782.0000 |

Manufacturer: MAICO

VEA ER 17/60-2 Fan insert with cover