**Tubular sound absorber RSR 25-1**

Tubular sound absorber for ventilation systems.

With sound absorbing packing made of synthetic resin-bonded glass fibres.

Non-combustible in accordance with DIN 4102 class A1 (building material classification).

Insertion loss measured in accordance with DIN 45646.

With lip seal.

Temperature resistant up to +70 °C.

RSR...: With 25 mm thick sound absorbing packing.

RSR.../50: With 50 mm thick sound absorbing packing.

Technical data

|  |  |
| --- | --- |
| Article: | RSR 25-1 |
| Model: | 25 mm sound absorbing cover |
| Installation site: | Fans |
| Material: | Aluminium |
| Colour: | Silver |
| Weight: | 1,95 kg |
| Weight including packaging: | 2,71 kg |
| Connection diameter: | 250 mm |
| Suitable for nominal size: | 250 mm |
| Width: | 310 mm |
| Height: | 310 mm |
| Depth: | 1.000 mm |
| Width with packaging: | 320 mm |
| Height with packaging: | 350 mm |
| Depth with packaging: | 1.175 mm |
| Insertion loss at 63 Hz: | 1 dB |
| Insertion loss at 125 Hz: | 1 dB |
| Insertion loss at 250 Hz: | 3 dB |
| Insertion loss at 500 Hz: | 7 dB |
| Insertion loss at 1 kHz: | 19 dB |
| Insertion loss at 2 kHz: | 18 dB |
| Insertion loss at 4 kHz: | 9 dB |
| Insertion loss at 8 kHz: | 13 dB |
| Sound insulation: | yes |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799925989 |
| Article number: | 0092.0598 |

Manufacturer: MAICO

RSR 25-1 Tubular sound absorber