**Recessed-mounted housing ER GH-VWR**

Special features

Model for front wall register construction.

With extension frame (40 mm deep).

Exhaust socket can be converted, without tools, from “side” to “rear”.

Lateral mounting grooves for installation with mounting brackets or in front wall installations.

Airstream-operated plastic backflow preventer with simultaneous function as a cold smoke barrier.

For applications in accordance with DIN 18017-3.

Single-room air extraction

Installation in bathrooms, WCs and open-plan kitchens.

For use in front wall register construction with a 40 mm extension frame.

6 laterally attached mounting grooves allow for easy installation.

Circumferential frame allows for additional fixing options.

Flexible cable entry allows electrical connection from the side or rear.

Simple electrical wiring on practical pin connector terminal.

With plaster protective cover to close the housing during the shell construction phase.

Plastic exhaust socket with airstream-operated plastic backflow preventer can be converted, without tools, for air outlet direction to the side (top, left, right) and rear.

DN 75/80 connection diameter.

Knockout points for second room connection or WC connection socket, as a standard feature, in the ER GH-VWR housing.

Certificates of approval on request or on our website – www.maico-ventilatoren.com.

Plastic parts, normally inflammable, according to DIN 4102-1 class B 2 (according to EN 13501-1).

Optional accessories

ER-AS extraction socket for the toilet seat air extraction

ER-ZR second room connection

ER-MS installation kit

ER-UPM mounting support

Technical data

|  |  |
| --- | --- |
| Article: | ER GH-VWR |
| Model: | Model for front wall register construction, plastic exhaust socket, convertible to the side/rear, with airstream-operated plastic backflow preventer, without fire protection housing, second room connection possible on right/left/at bottom |
| Air direction: | Air extraction |
| Installation site: | Wall / ceiling |
| Material: | Plastic / metal |
| Colour: | Black / galvanized |
| Weight: | 0,87 kg |
| Weight including packaging: | 1,19 kg |
| Air outlet direction: | at side / at rear |
| Connection diameter: | 75 mm / 80 mm |
| Width: | 280 mm |
| Height: | 133 mm |
| Depth: | 343 mm |
| Width with packaging: | 320 mm |
| Height with packaging: | 190 mm |
| Depth with packaging: | 420 mm |
| Packing unit: | 1 piece |
| Range: | B |
| GTIN (EAN): | 4012799992349 |
| Article number: | 0093.1564 |

Manufacturer: MAICO

ER GH-VWR Recessed-mounted housing