**Channel shutter AKP 22**

Shutters for air extraction.

With galvanised protective grille.

Installation instructions

Check to make sure the shutter cannot be accessed when installing in potentially explosive atmospheres.

If it can be touched, pull a finely machined wire cage across the shutter.

Securely earth the wire cage in order to prevent sparks.

Technical data

|  |  |
| --- | --- |
| Article: | AKP 22 |
| Air direction: | Air extraction |
| Loss of pressure: | 10 Pa |
| Installation: | outside |
| Installation site: | Channel |
| Installation position: | vertical / horizontal |
| Material: | Synthetic material, weather and UV resistant |
| Colour: | Light grey |
| Weight: | 1,24 kg |
| Weight including packaging: | 1,61 kg |
| Type of shutter: | Airstream-operated opening/closing |
| Channel dimension: | 500 mm x 250 mm |
| Width: | 335 mm |
| Height: | 585 mm |
| Depth: | 54 mm |
| Width with packaging: | 350 mm |
| Height with packaging: | 610 mm |
| Depth with packaging: | 60 mm |
| Ambient temperature: | 60 °C |
| Packing unit: | 1 piece |
| Range: | D |
| GTIN (EAN): | 4012799510963 |
| Article number: | 0151.0096 |

Manufacturer: MAICO

AKP 22 Channel shutter