**Wall frame ER-MR EC**

Wall frames for housings that have been plastered too deep, to prevent the air from being drawn out of the shaft.

Combination with ER GH housing possible.

Made from cement-bonded polystyrene structural panels which can be individually shortened.

Can be shortened to depth of between 75 mm and 15 mm.

With 55/80 mm screw.

Technical data

|  |  |
| --- | --- |
| Article: | ER-MR EC |
| Type of installation: | Recessed-mounted |
| Material: | Polystyrene, cement-bonded |
| Colour: | grey |
| Weight: | 0,27 kg |
| Weight including packaging: | 0,51 kg |
| Width: | 265 mm |
| Height: | 265 mm |
| Depth: | 75 mm |
| Width with packaging: | 695 mm |
| Height with packaging: | 85 mm |
| Depth with packaging: | 85 mm |
| Packing unit: | 1 piece |
| Range: | B |
| GTIN (EAN): | 4012799927655 |
| Article number: | 0192.0765 |

Manufacturer: MAICO

ER-MR EC Wall frame