**Masking frame ER-AR EC**

Cover frame for ER GH and ER GH-VWR flush-mounted housing, for flush-mounted housing that is not installed deeply enough and for large joint gaps.

Max. depth 35 mm.

Covers joint between the flush-mounted housing and wall tiles.

Prevents unattractive gaps around the flush-mounted housing.

Insert the cover frame between the wall and the internal cover.

Technical data

|  |  |
| --- | --- |
| Article: | ER-AR EC |
| Installation: | Inside |
| Type of installation: | Surface-mounted |
| Material: | Synthetic material |
| Colour: | Traffic white, similar to RAL 9016 |
| Weight: | 0,2 kg |
| Weight including packaging: | 0,38 kg |
| Width: | 307 mm |
| Height: | 307 mm |
| Depth: | 35 mm |
| Width with packaging: | 335 mm |
| Height with packaging: | 335 mm |
| Depth with packaging: | 60 mm |
| Packing unit: | 1 piece |
| Range: | B |
| GTIN (EAN): | 4012799932765 |
| Article number: | 0093.0276 |

Manufacturer: MAICO

ER-AR EC Masking frame