**Channel shutter RKP 25**

Technical data

|  |  |
| --- | --- |
| Article: | RKP 25 |
| Air direction: | Ventilation and air extraction |
| Installation site: | Channel |
| Installation position: | vertical / horizontal |
| Material: | Sheet steel, galvanised |
| Weight: | 5,275 kg |
| Weight including packaging: | 5,47 kg |
| Type of shutter: | electrical |
| Channel dimension: | 500 mm x 300 mm |
| Width: | 540 mm |
| Height: | 340 mm |
| Depth: | 120 mm |
| Width with packaging: | 640 mm |
| Height with packaging: | 340 mm |
| Depth with packaging: | 130 mm |
| Packing unit: | 1 piece |
| Range: | D |
| GTIN (EAN): | 4012799512363 |
| Article number: | 0151.0236 |

Manufacturer:
MAICO

RKP 25 Channel shutter