**Cleaning opening with O-ring gasket RO 180**

Technical data

|  |  |
| --- | --- |
| Article: | RO 180 |
| Type of installation: | Recessed-mounted |
| Ambient temperature: | 60 °C |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799924104 |
| Article number: | 0092.0410 |

Manufacturer: MAICO

RO 180 Cleaning opening with O-ring gasket