**Greenhouse fan EFG 20 E**

Technical data

|  |  |
| --- | --- |
| Article: | EFG 20 E |
| Air flow volume: | 330 m³/h |
| Rotating speed: | 1.400 1/min |
| Reversing capacity: | - |
| Nominal output: | 30 W |
| Power consumption: | 33 W |
| Inom: | 0,24 A |
| Imax: | 0,24 A |
| Degree of protection: | IP X4 |
| Weight: | 4,81 |
| Nominal size: | 200 mm |
| Airstream temperature at nominal current: | 60 °C |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799814016 |
| Article number: | 0081.0401 |

Manufacturer: MAICO

EFG 20 E Greenhouse fan