**Fan insert ER 17 G**

Technical data

|  |  |
| --- | --- |
| Article: | ER 17 G |
| Model: | Base load circuit |
| Air flow volume: | 21 m³/h / 61 m³/h |
| Rotating speed: | 1.000 1/min / 2.650 1/min |
| Speed controllable: | - |
| Rated voltage: | 230 V |
| Power consumption: | 33 W / 55 W |
| Imax: | 0,28 A / 0,36 A |
| Installation site: | Ceiling / Wall |
| Type of installation: | Recessed-mounted |
| Installation position: | any |
| Weight: | 2,4 |
| Nominal size: | 75 mm |
| Packing unit: | 1 piece |
| Article number: | 0080.0238 |

Manufacturer: MAICO

ER 17 G Fan insert