**Small room fan ECA 10-2 VZ**

Technical data

|  |  |
| --- | --- |
| Article: | ECA 10-2 VZ |
| Model: | Time delay switch |
| Air flow volume: | 150 m³/h |
| Rotating speed: | 2.600 1/min |
| Type of voltage: | Alternating current |
| Rated voltage: | 230 V |
| Power consumption: | 18 W |
| Imax: | 0,13 A |
| Degree of protection: | IP 44 |
| Installation site: | Wall / Ceiling |
| Installation position: | any |
| Material: | Synthetic material |
| Colour: | Traffic white, similar to RAL 9016 |
| Pulley integrated: | ✔ |
| Packing unit: | 1 piece |
| Article number: | 080019 |

Manufacturer: MAICO

ECA 10-2 VZ Small room fan