**Flexible duct MF-F90**

Particularly flexible ducts.

Specially developed for ventilation applications.

Odour-neutral and with anti-static treatment.

Low flow resistance with good sound deadening.

Hygienic.

Few dirt deposits.

Duct is corrugated on outside.

Simple installation because the duct's flexibility allows it to be moved between the air distributor and supply air or exhaust air valve.

Technical data

|  |  |
| --- | --- |
| Article: | MF-F90 |
| Air direction: | Ventilation and air extraction |
| Volumetric flow: | 50 m³/h recommended |
| Installation site: | Ceiling / Floor / Wall |
| Material: | Polyethylene (PE) |
| Synthetic material definition: | PVC-free |
| Fire behaviour: | Normally inflammable building material (fire behaviour E according to DIN EN 13501-1: 2010) |
| Annular rigidity: | ≥ 8 kN/m² in accordance with EN ISO 9969 |
| Weight: | 23 kg |
| Weight including packaging: | 23,5 kg |
| Nominal size: | 90 mm |
| Internal diameter: | 77,5 mm |
| Length: | 50 m |
| Width: | 90 mm |
| Height: | 90 mm |
| Depth: | 50.000 mm |
| Width with packaging: | 1.302 mm |
| Height with packaging: | 452 mm |
| Depth with packaging: | 1.302 mm |
| Minimum bend radius: | 350 mm |
| Ambient temperature: | -20 °C up to 60 °C |
| Packing unit: | 1 x 50 m roll |
| Range: | K |
| GTIN (EAN): | 4012799550952 |
| Article number: | 0055.0095 |

Manufacturer: MAICO

MF-F90 Flexible duct