**Floor / wall outlet MF-FBWA 75**

Floor and wall outlet for MAICOFlex flexible ventilation duct system

For connecting 2 MF-F flexible steel ducts.

Stainless steel air grille with slotted look.

Simple regulation using inbuilt air volume slide with lock, including telescopic element for extension when fitted in concrete ceiling.

The mounting height between the bottom of the basic element and the top of the stainless steel grille (total height) can be variably set between 13 cm and 29 cm.

Accessories needed: Two MF-FDR gaskets.

Technical data

|  |  |
| --- | --- |
| Article: | MF-FBWA 75 |
| Air direction: | Ventilation |
| Volumetric flow: | 40 m³/h recommended |
| Grille material: | Stainless steel |
| Housing material: | Sheet steel, Sendzimir galvanised |
| Weight: | 3,31 kg |
| Weight including packaging: | 3,71 kg |
| Nominal size: | 75 mm |
| Width: | 330 mm |
| Height: | 290 mm |
| Depth: | 130 mm |
| Width with packaging: | 395 mm |
| Height with packaging: | 260 mm |
| Depth with packaging: | 200 mm |
| Sound power level: | 24 dB(A) / at 50 m³/h |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799520665 |
| Article number: | 0152.0066 |

Manufacturer: MAICO

MF-FBWA 75 Floor / wall outlet