**Room air control RLS 4-1 UP**

Room air control for WRG 35 single-room ventilation unit.

The controller is needed as an accessory for the WRG 35-1-SE final assembly kit.

Accessories supplied: 5 m connecting duct.

RLS 4-1 room air control features the following setting options:

The filter change display interval can be set to between 2 and 9 months.

The zero ventilation level can be deactivated as a result of which the fans operate continually.

Up to a maximum of 9 units can be controlled at the same time through an RLS 4-1 room air control.

Technical data

|  |  |
| --- | --- |
| Article: | RLS 4-1 UP |
| Speed controllable: | - |
| Degree of protection: | IP 00 |
| Type of installation: | Recessed-mounted |
| Installation position: | any |
| Material: | Synthetic material |
| Colour: | White |
| Weight: | 0,1 kg |
| Weight including packaging: | 0,224 kg |
| Width: | 80 mm |
| Height: | 80 mm |
| Depth: | 20 mm |
| Width with packaging: | 225 mm |
| Height with packaging: | 95 mm |
| Depth with packaging: | 115 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799578482 |
| Article number: | 0157.0848 |

Manufacturer: MAICO

RLS 4-1 UP Room air control