**Exhaust socket with pre-assembled backflow preventer ABSM RK ER-UPD/-UPB**

Exhaust socket with pre-assembled metal backflow preventer as spare part for various recessed-mounted housing the ER-UPD and ER-UPB groups.

Technical data

|  |  |
| --- | --- |
| Article: | ABSM RK ER-UPD/-UPB |
| Housing material: | Metal |
| Colour: | Silver |
| Weight: | 0,26 kg |
| Weight including packaging: | 0,36 kg |
| Width: | 85 mm |
| Height: | 82 mm |
| Depth: | 85 mm |
| Width with packaging: | 170 mm |
| Height with packaging: | 155 mm |
| Depth with packaging: | 170 mm |
| Range: | B |
| GTIN (EAN): | 4012799100140 |
| Article number: | E093.0977.0001 |

Manufacturer:

 MAICO

ABSM RK ER-UPD/-UPB Exhaust socket with pre-assembled backflow preventer