**Additional circuit board ZP 1**

The ZP 1 additional circuit board is used to control optional components, e.g.

to control a 3-way shutter for air-earth heat exchangers

to control a controlled pump for a brine earth heat exchanger

to control an air shutter for zone control

used as a switching contact for external postheating register

Communication between the basic PCB and additional board ZP 1 is established via the RJ 12 modular cable supplied.

The desired function can be selected via the Dip switch on the ZP 1.

For WS 120 Trio, WS 160 Flat, WS 170, WS 300 Flat, WR 310 / WR 410, WS 320 and WS 470 centralised ventilation units.

Technical data

|  |  |
| --- | --- |
| Article: | ZP 1 |
| Weight: | 0,08 kg |
| Weight including packaging: | 0,18 kg |
| Width: | 71 mm |
| Height: | 77 mm |
| Depth: | 83 mm |
| Width with packaging: | 170 mm |
| Height with packaging: | 83 mm |
| Depth with packaging: | 160 mm |
| Packing unit: | 1 piece |
| Suitable for products: | WS 160 Flat, WS 170 KB.., WS 320, WS 470, WR 310, WR 410 |
| Range: | K |
| GTIN (EAN): | 4012799925545 |
| Article number: | 0092.0554 |

Manufacturer: MAICO

ZP 1 Additional circuit board